**Machine learning-assisted exploration for carbon neutrality potential of municipal sludge recycling *via* hydrothermal carbonization**

Xinzhe Zhu a,b, Bingyou Liu a,b, Lianpeng Suna,b\*, Ruohong Lia,b, Huanzhong Denga,b, Xiefei Zhuc,d, Daniel C.W. Tsang c

a School of Environmental Science and Engineering, Sun Yat-sen University, Guangzhou 510275, China

b Guangdong Provincial Key Laboratory of Environmental Pollution Control and Remediation Technology, Sun Yat-sen University, Guangzhou 510275, China

c Department of Civil and Environmental Engineering, The Hong Kong Polytechnic University, Hung Hom, Kowloon, Hong Kong, China

d Department of Thermal Science and Energy Engineering, University of Science and Technology of China, 96 Jinzhai Road, Hefei, Anhui 230026, China

\*Corresponding author email: [eesslp@mail.sysu.edu.cn](mailto:eesslp@mail.sysu.edu.cn)

# **References**

Ahn, H., Kim, D., Lee, Y. 2020. Combustion characteristics of sewage sludge solid fuels produced by drying and hydrothermal carbonization in a fluidized bed. *Renew. Energ.*, **147**, 957-968.

Alipour, M., Asadi, H., Chen, C., Rashti, M.R. 2021. Bioavailability and eco-toxicity of heavy metals in chars produced from municipal sewage sludge decreased during pyrolysis and hydrothermal carbonization. *Ecol. Eng.*, **162**. 106173

Aragón-Briceño, C., Ross, A.B., Camargo-Valero, M.A. 2017. Evaluation and comparison of product yields and bio-methane potential in sewage digestate following hydrothermal treatment. *Appl. Energ.*, **208**, 1357-1369.

Aragón-Briceño, C.I., Grasham, O., Ross, A.B., Dupont, V., Camargo-Valero, M.A. 2020. Hydrothermal carbonization of sewage digestate at wastewater treatment works: Influence of solid loading on characteristics of hydrochar, process water and plant energetics. *Renew. Energ.*, **157**, 959-973.

Aragón-Briceño, C.I., Ross, A.B., Camargo-Valero, M.A. 2021. Mass and energy integration study of hydrothermal carbonization with anaerobic digestion of sewage sludge. *Renew. Energ.*, **167**, 473-483.

Arauzo, P.J., Atienza-Martínez, M., Ábrego, J., Olszewski, M.P., Cao, Z., Kruse, A. 2020. Combustion Characteristics of Hydrochar and Pyrochar Derived from Digested Sewage Sludge. *Energies*, **13**(16).

Atallah, E., Kwapinski, W., Ahmad, M.N., Leahy, J.J., Zeaiter, J. 2019. Effect of water-sludge ratio and reaction time on the hydrothermal carbonization of olive oil mill wastewater treatment: Hydrochar characterization. *J. Water. Process. Eng.*, **31**.

Becker, G.C., Wust, D., Kohler, H., Lautenbach, A., Kruse, A. 2019. Novel approach of phosphate-reclamation as struvite from sewage sludge by utilising hydrothermal carbonization. *J. Environ. Manage.*, **238**, 119-125.

Belete, Y.Z., Leu, S., Boussiba, S., Zorin, B., Posten, C., Thomsen, L., Wang, S., Gross, A., Bernstein, R. 2019. Characterization and utilization of hydrothermal carbonization aqueous phase as nutrient source for microalgal growth. *Bioresour. Technol.*, **290**, 121758.

Bhatt, D., Shrestha, A., Dahal, R., Acharya, B., Basu, P., MacEwen, R. 2018. Hydrothermal Carbonization of Biosolids from Waste Water Treatment Plant. *Energies*, **11**(9).

Breulmann, M., van Afferden, M., Müller, R.A., Schulz, E., Fühner, C. 2017. Process conditions of pyrolysis and hydrothermal carbonization affect the potential of sewage sludge for soil carbon sequestration and amelioration. *J. Anal. Appl. Pyrol.*, **124**, 256-265.

Danso-Boateng, E., Holdich, R.G., Shama, G., Wheatley, A.D., Sohail, M., Martin, S.J. 2013. Kinetics of faecal biomass hydrothermal carbonisation for hydrochar production. *Appl. Energ.*, **111**, 351-357.

Danso-Boateng, E., Shama, G., Wheatley, A.D., Martin, S.J., Holdich, R.G. 2015. Hydrothermal carbonisation of sewage sludge: effect of process conditions on product characteristics and methane production. *Bioresour. Technol.*, **177**, 318-27.

Escala, M., Zumbühl, T., Koller, C., Junge, R., Krebs, R. 2012. Hydrothermal Carbonization as an Energy-Efficient Alternative to Established Drying Technologies for Sewage Sludge: A Feasibility Study on a Laboratory Scale. *Energ. Fuel.*, **27**(1), 454-460.

Fei, Y.H., Zhao, D., Liu, Y., Zhang, W., Tang, Y.Y., Huang, X., Wu, Q., Wang, Y.X., Xiao, T., Liu, C. 2019. Feasibility of sewage sludge derived hydrochars for agricultural application: Nutrients (N, P, K) and potentially toxic elements (Zn, Cu, Pb, Ni, Cd). *Chemosphere*, **236**, 124841.

Ferrentino, R., Ceccato, R., Marchetti, V., Andreottola, G., Fiori, L. 2020. Sewage Sludge Hydrochar: An Option for Removal of Methylene Blue from Wastewater. *Appl. Sci.*, **10**(10).

Filipowicz, M., Wilk, M., Dudek, M., Olkuski, T., Styszko, K. 2016. A novel method of sewage sludge pre-treatment - HTC. *E3S Web of Conferences*, **10**, 00103

Gai, C., Chen, M., Liu, T., Peng, N., Liu, Z. 2016. Gasification characteristics of hydrochar and pyrochar derived from sewage sludge. *Energy*, **113**, 957-965.

Gao, N., Li, Z., Quan, C., Miskolczi, N., Egedy, A. 2019. A new method combining hydrothermal carbonization and mechanical compression in-situ for sewage sludge dewatering: Bench-scale verification. *J. Anal. Appl. Pyrol.*, **139**, 187-195.

Hamalainen, A., Kokko, M., Kinnunen, V., Hilli, T., Rintala, J. 2022. Hydrothermal carbonization of pulp and paper industry wastewater treatment sludges - characterization and potential use of hydrochars and filtrates. *Bioresour. Technol.*, **355**, 127258.

He, C., Giannis, A., Wang, J.-Y. 2013. Conversion of sewage sludge to clean solid fuel using hydrothermal carbonization: Hydrochar fuel characteristics and combustion behavior. *Appl. Energ.*, **111**, 257-266.

He, C., Zhang, Z., Ge, C., Liu, W., Tang, Y., Zhuang, X., Qiu, R. 2019. Synergistic effect of hydrothermal co-carbonization of sewage sludge with fruit and agricultural wastes on hydrochar fuel quality and combustion behavior. *Waste Manag.*, **100**, 171-181.

Huezo, L., Vasco-Correa, J., Shah, A. 2021. Hydrothermal carbonization of anaerobically digested sewage sludge for hydrochar production. *Bioresour. Technol. Report*, **15**,100795

Khoshbouy, R., Takahashi, F., Yoshikawa, K. 2019. Preparation of high surface area sludge-based activated hydrochar via hydrothermal carbonization and application in the removal of basic dye. *Environ. Res.*, **175**, 457-467.

Kim, D., Lee, K., Park, K.Y. 2014. Hydrothermal carbonization of anaerobically digested sludge for solid fuel production and energy recovery. *Fuel*, **130**, 120-125.

Kim, D., Park, S., Park, K.Y. 2017. Upgrading the fuel properties of sludge and low rank coal mixed fuel through hydrothermal carbonization. *Energy*, **141**, 598-602.

Lee, J., Sohn, D., Lee, K., Park, K.Y. 2019. Solid fuel production through hydrothermal carbonization of sewage sludge and microalgae Chlorella sp. from wastewater treatment plant. *Chemosphere*, **230**, 157-163.

Li, C., Li, J., Xie, S., Zhang, G., Pan, L., Wang, R., Wang, G., Pan, X., Wang, Y., Angelidaki, I. 2022. Enhancement of heavy metal immobilization in sewage sludge biochar by combining alkaline hydrothermal treatment and pyrolysis. *J. Clean. Prod.*, **369**.133325

Li, C., Wang, X., Zhang, G., Yu, G., Lin, J., Wang, Y. 2017. Hydrothermal and alkaline hydrothermal pretreatments plus anaerobic digestion of sewage sludge for dewatering and biogas production: Bench-scale research and pilot-scale verification. *Water Res.*, **117**, 49-57.

Li, Y., Yang, X., Zhu, M., Dong, L., Jiang, H., Xu, Q., Zhou, H., Han, Y., Feng, L., Li, C. 2022. Synergistic effect of combined hydrothermal carbonization of Fenton's reagent and biomass enhances the adsorption and combustion characteristics of sludge towards eco-friendly and efficient sludge treatment. *Sci. Total. Environ.*, **825**, 153854.

Liu, M., Duan, Y., Bikane, K., Zhao, L. 2017. Effect of waste liquid produced from the hydrothermal treatment of both low-rank coal and sludge on the slurryability of coal sludge slurry. *Fuel*, **203**, 1-10.

Liu, T., Guo, Y., Peng, N., Lang, Q., Xia, Y., Gai, C., Zheng, Q., Liu, Z. 2018. Identification and quantification of polycyclic aromatic hydrocarbons generated during pyrolysis of sewage sludge: Effect of hydrothermal carbonization pretreatment. *J. Anal. Appl. Pyrol.*, **130**, 99-105.

Liu, T., Lang, Q., Xia, Y., Chen, Z., Li, D., Ma, J., Gai, C., Liu, Z. 2019. Combination of hydrothermal carbonization and oxy-fuel combustion process for sewage sludge treatment: Combustion characteristics and kinetics analysis. *Fuel*, **242**, 265-276.

Liu, W., Zheng, X., Ying, Z., Feng, Y., Wang, B., Dou, B. 2022. Hydrochar prepared from municipal sewage sludge as renewable fuels: Evaluation of its devolatilization performance, reaction mechanism, and thermodynamic property. *J. Environ. Chem. Eng.*, **10**(5).

Liu, X., Zhai, Y., Li, S., Niu, Q., Liu, X., Wang, Z., Liu, Y., Qiu, Z., Li, C., Zhu, Y., Xu, M. 2022. Hydrothermal carbonization of petrochemical sludge: The fate of hydrochar and oil components. *J. Environ. Chem. Eng.*, **10**(5).

Ma, J., Chen, M., Yang, T., Liu, Z., Jiao, W., Li, D., Gai, C. 2019. Gasification performance of the hydrochar derived from co-hydrothermal carbonization of sewage sludge and sawdust. *Energy*, **173**, 732-739.

Malhotra, M., Garg, A. 2020. Hydrothermal carbonization of centrifuged sewage sludge: Determination of resource recovery from liquid fraction and thermal behaviour of hydrochar. *Waste Manag.*, **117**, 114-123.

Marin-Batista, J.D., Mohedano, A.F., Rodriguez, J.J., de la Rubia, M.A. 2020. Energy and phosphorous recovery through hydrothermal carbonization of digested sewage sludge. *Waste Manag.*, **105**, 566-574.

Medina-Martos, E., Istrate, I.-R., Villamil, J.A., Gálvez-Martos, J.-L., Dufour, J., Mohedano, Á.F. 2020. Techno-economic and life cycle assessment of an integrated hydrothermal carbonization system for sewage sludge. *J. Clean. Prod.*, **277**. 122930

Merzari, F., Goldfarb, J., Andreottola, G., Mimmo, T., Volpe, M., Fiori, L. 2020. Hydrothermal Carbonization as a Strategy for Sewage Sludge Management: Influence of Process Withdrawal Point on Hydrochar Properties. *Energies*, **13**(11).

Mittapalli, S., Sharma, H.B., Dubey, B.K. 2021. Hydrothermal carbonization of anaerobic granular sludge and co-pelletization of hydrochar with yard waste. *Bioresour. Technol. Reports*, **14**.100691

Oliveira, A.S., Sarrión, A., Baeza, J.A., Diaz, E., Calvo, L., Mohedano, A.F., Gilarranz, M.A. 2022. Integration of hydrothermal carbonization and aqueous phase reforming for energy recovery from sewage sludge. *Chem. Eng. J.*, **442**.136301

Paneque, M., De la Rosa, J.M., Kern, J., Reza, M.T., Knicker, H. 2017. Hydrothermal carbonization and pyrolysis of sewage sludges: What happen to carbon and nitrogen? *J. Anal. Appl. Pyrol.*, **128**, 314-323.

Parmar, K.R., Ross, A.B. 2019. Integration of Hydrothermal Carbonisation with Anaerobic Digestion; Opportunities for Valorisation of Digestate. *Energies*, **12**(9).

Peng, C., Zhai, Y., Zhu, Y., Xu, B., Wang, T., Li, C., Zeng, G. 2016. Production of char from sewage sludge employing hydrothermal carbonization: Char properties, combustion behavior and thermal characteristics. *Fuel*, **176**, 110-118.

Qi, G., Wang, X., Shen, Y., Liu, X., Asraful Alam, M., Liu, B., Chen, Y. 2022. Effect of different flocculants on the characteristics of hydrochar and hydroliquid derived from the hydrothermal treated active sludge. A comparative study. *J. Environ. Chem. Eng.*, **10**(3).

Sarrion, A., de la Rubia, A., Coronella, C., Mohedano, A.F., Diaz, E. 2022. Acid-mediated hydrothermal treatment of sewage sludge for nutrient recovery. *Sci. Total Environ.*, **838**(Pt 4), 156494.

Silva, R.D.V.K., Lei, Z., Shimizu, K., Zhang, Z. 2020. Hydrothermal treatment of sewage sludge to produce solid biofuel: Focus on fuel characteristics. *Bioresour. Technol. Reports*, **11**. 100453

Smith, A.M., Singh, S., Ross, A.B. 2016. Fate of inorganic material during hydrothermal carbonisation of biomass: Influence of feedstock on combustion behaviour of hydrochar. *Fuel*, **169**, 135-145.

Song, E., Park, S., Kim, H. 2019. Upgrading Hydrothermal Carbonization (HTC) Hydrochar from Sewage Sludge. *Energies*, **12**(12).

Villamil, J.A., Mohedano, A.F., Rodriguez, J.J., De la Rubia, M.A. 2019. Anaerobic co-digestion of the aqueous phase from hydrothermally treated waste activated sludge with primary sewage sludge. A kinetic study. *J. Environ. Manage.*, **231**, 726-733.

Villamil, J.A., Mohedano, A.F., San Martín, J., Rodriguez, J.J., de la Rubia, M.A. 2020. Anaerobic co-digestion of the process water from waste activated sludge hydrothermally treated with primary sewage sludge. A new approach for sewage sludge management. *Renew. Energ.*, **146**, 435-443.

Wang, C., Zhu, W., Fan, X. 2021. Char derived from sewage sludge of hydrothermal carbonization and supercritical water gasification: Comparison of the properties of two chars. *Waste Manag.*, **123**, 88-96.

Wang, R., Wang, C., Zhao, Z., Jia, J., Jin, Q. 2019. Energy recovery from high-ash municipal sewage sludge by hydrothermal carbonization: Fuel characteristics of biosolid products. *Energy*, **186**. 115848

Wang, S., Persson, H., Yang, W., Jönsson, P.G. 2020. Pyrolysis study of hydrothermal carbonization-treated digested sewage sludge using a Py-GC/MS and a bench-scale pyrolyzer. *Fuel*, **262**.116335

Wang, X., Shen, Y., Liu, X., Ma, T., Wu, J., Qi, G. 2022. Fly ash and H2O2 assisted hydrothermal carbonization for improving the nitrogen and sulfur removal from sewage sludge. *Chemosphere*, **290**, 133209.

Wang, Z., Zhai, Y., Wang, T., Peng, C., Li, S., Wang, B., Liu, X., Li, C. 2020. Effect of temperature on the sulfur fate during hydrothermal carbonization of sewage sludge. *Environ. Pollut.*, **260**, 114067.

Wilk, M., Magdziarz, A., Jayaraman, K., Szymańska-Chargot, M., Gökalp, I. 2019. Hydrothermal carbonization characteristics of sewage sludge and lignocellulosic biomass. A comparative study. *Biomass. Bioenerg.*, **120**, 166-175.

Yu, Y., Lei, Z., Yang, X., Yang, X., Huang, W., Shimizu, K., Zhang, Z. 2018. Hydrothermal carbonization of anaerobic granular sludge: Effect of process temperature on nutrients availability and energy gain from produced hydrochar. *Appl. Energ.*, **229**, 88-95.

Zhang, X.-P., Zhang, C., Li, X., Yu, S.-H., Tan, P., Fang, Q.-Y., Chen, G. 2018. A two-step process for sewage sludge treatment: Hydrothermal treatment of sludge and catalytic hydrothermal gasification of its derived liquid. *Fuel Process. Technol.*, **180**, 67-74.

Zhao, J., Liu, C., Hou, T., Lei, Z., Yuan, T., Shimizu, K., Zhang, Z. 2022. Conversion of biomass waste to solid fuel via hydrothermal co-carbonization of distillers grains and sewage sludge. *Bioresour. Technol.*, **345**, 126545.

Zhao, P., Shen, Y., Ge, S., Yoshikawa, K. 2014. Energy recycling from sewage sludge by producing solid biofuel with hydrothermal carbonization. *Energ. Convers. Manage.*, **78**, 815-821.

Zheng, C., Ma, X., Yao, Z., Chen, X. 2019. The properties and combustion behaviors of hydrochars derived from co-hydrothermal carbonization of sewage sludge and food waste. *Bioresour. Technol.*, **285**, 121347.

Zheng, X., Huang, J., Ying, Z., Ji, S., Feng, Y., Wang, B., Dou, B. 2021. Thermochemical conversion of sewage sludge-derived hydrochars: Volatiles release and char gasification kinetics. *J. Anal. Appl. Pyrol.*, **156**.105138